**TELEVISION (DISPLAY TECHNOLOGIES)**

|  |  |
| --- | --- |
| accelerate | pospeševati |
| active-matrix | prikazovalnik z aktivno matriko |
| address electrode | elektroda naslova/naslovna elektroda ?? |
| align | poravnati v vrsto |
| anode connection | Anodni priključek |
| aspect ratio | razmerje gledišča | |
| brightness | sijaj, sijajnost |
| broadcast format | oddani format | |
| coating | prevleka |
| CRT (cathode-ray tube) | katodna cev |
| cutaway | presek |
| deflect | odbiti, odkloniti |
| deflection | odklon |
| deflection coil | odklonska tuljava |
| dielectric layer | neprevodni sloj |
| display electrode | prikazovalna elektroda |
| DTV (digital telvision) | digitalna televizija |
| electromagnetic focus | elektromagnetno žarišče |
| electron beam | elektronski snop |
| electron gun | elektronski top |
| emit light | oddajati svetlobo |
| etched | jedkan |
| evacuated glass envelope | nepredušna steklena posoda |
| filter film | tanek sloj, tanek film |
| flat panel tv | televizija z ravnim ekranom |
| focusing coil | žariščna tuljava |
| frame | slika, okvir, |
| frame rate | hitrost slike | |
| front plate glass | prednja steklena plošča |
| give off | oddajati |
| glass substrate | stekleni substrat |
| HDTV (high definition television) | visoko ločljiva televizija |
| image | slika |
| interlaced | prepleten |
| ito electrode | ito elektroda |
| LCD (liquid crystal display ) | prikazovalnik s tekočim kristalom |
| liquid crystal solution | izdelek/izvedba s tekočim kristalom |
| magnesium oxide coating | prevleka iz magnezijevega oksida |
| magnetic deflection | magnetni odklon |
| magnetic yoke | elektromagnetni jarem |
| mask | maska, prevleka |
| matrix electrode configuration | zgradba matrike z elektrodo |
| monochrome | monokromatski |
| nematic | nitast, vlaknast |
| noble gas | žlahtni plin |
| outgassing | izhajanje plina |
| pan and scan | slikovno drsenje in analiziranje | |
| panning | slikovno drsenje | |
| scanning | analiziranje slike | |
| passage of light | prehod svetlobe |
| passive-matriex | prikaz s pasivni matriko |
| PDP (plasma display panel) | plazma ekran |
| phosphor-coated | prevlečen s fosforjem |
| pixel | pika |
| plasma cell | plazma celica |
| plasma tv | plasma televzija |
| polarized light | polarizirana svetloba |
| polarizing filter | polarizacijski filter |
| poorly conductive | slabo prevoden |
| portion | predel |
| progressive | postopen |
| progressive scan | postopno analiziranje |
| raster | raster, slikovni vzorec |
| rear plate glass | steklo na zadnji plošči |
| render | odstopiti |
| repel | odbiti se |
| resolution | ločljivost | |
| ridge | greben, sleme, hrbet |
| SDTV (standard television) | klasična televizija |
| shadow-mask crt | senčna maska (slikovne elektronke) |
| sticking | sunek, lepljenje |
| subpixel | podpika |
| thermionic emission | termionično oddajanje |
| thin beam | tanek snop |
| transition metal | prehodna kovina |
| triad | triada |
| vaccum tube | elektronka |

**TELEVISION (DISPLAY TECHNOLOGIES)**

|  |  |
| --- | --- |
| accelerate |  |
| active-matrix |  |
| address electrode |  |
| align |  |
| anode connection |  |
| aspect ratio |  | |
| brightness |  |
| broadcast format |  | |
| coating |  |
| CRT (cathode-ray tube) |  |
| cutaway |  |
| deflect |  |
| deflection |  |
| deflection coil |  |
| dielectric layer |  |
| display electrode |  |
| DTV (digital telvision) |  |
| electromagnetic focus |  |
| electron beam |  |
| electron gun |  |
| emit light |  |
| etched |  |
| evacuated glass envelope |  |
| filter film |  |
| flat panel tv |  |
| focusing coil |  |
| frame |  |
| frame rate |  | |
| front plate glass |  |
| give off |  |
| glass substrate |  |
| HDTV (high definition television) |  |
| image |  |
| interlaced |  |
| ITO electrode |  |
| LCD (liquid crystal display ) |  |
| liquid crystal solution |  |
| magnesium oxide coating |  |
| magnetic deflection |  |
| magnetic yoke |  |
| mask |  |
| matrix electrode configuration |  |
| monochrome |  |
| nematic |  |
| noble gas |  |
| outgassing |  |
| pan and scan |  | |
| panning |  | |
| scanning |  | |
| passage of light |  |
| passive-matriex |  |
| PDP (plasma display panel) |  |
| phosphor-coated |  |
| pixel |  |
| plasma cell |  |
| plasma tv |  |
| polarized light |  |
| polarizing filter |  |
| poorly conductive |  |
| portion |  |
| progressive |  |
| progressive scan |  |
| raster |  |
| rear plate glass |  |
| render |  |
| repel |  |
| resolution |  | |
| ridge |  |
| SDTV (standard television) |  |
| shadow-mask crt |  |
| sticking |  |
| subpixel |  |
| thermionic emission |  |
| thin beam |  |
| transition metal |  |
| triad |  |
| vaccum tube |  |